Discussion1: After myservo.write(val), why do we need delay(15)? What will happen if we don’t use delay?

要等旋轉軸轉到那個位置，沒寫 delay 的話，可能在轉到指定的位置之前就又有新的指令。

Discussion2:

1. Study the code in BMP085.cpp. How does the altitude is calculated by using pressure?

44330 \* (1.0 - pow(pressure / seaLevelPressure, 0.1903));

1. What is the unit of the altitude formula? (as follows)

公尺

1. Try to lift your BMP180 sensor, and write down the value change between put it on the table and lift it up.

0.6(156.4-155.8)